DX100 Report program – Setting up channel 01 for a Hourly & Daily Report. 

1) Press STOP key to stop recording. We need to stop both Memory+Math. 
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2) Press MENU key.
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3) Press NEXT key 2 times. 
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4) Select #9, Option.  
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5) Select #2 Report
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6) Select HOUR+DAY 
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7) Scroll to Sum Scale. 
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8) Select /min for a flow that is based on minute example GPM. 
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9) Press DISP/Enter key so no Yellow highlight is showing. 
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10)Press ESC key until display looks like below. 
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11) Select Next 3/4key 
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12) Select END and press Enter key and let the recorder reboot.  
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13) Press DISP/Enter key. Select Information, Memory Summary. Press DISP/Enter key. 
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14) This is the screen that will show the Reports. If an existing Report has been completed it will be displayed as Report (01/05). You can STOP data collection and Restart it to force a Report for test purposes. 
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15) Press DISP/Enter key and select JUMP to REPORT. Press DISP/Enter key.
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16) If more then one Report is available you can Right and Left Arrow key to scroll.  
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17) Press Enter key.
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